**Electronic Expansion Valve Information**

**Version Follow List?**

**5 March 2013**

1) Log File Add ins for Max Step Limits

2) Log File Limited to 30 min ax log then log files as 001 002

**17:49:50..Nov 26 2012 to 09:46:02..Nov 27 2012**

1) Thermal Cut ON/OFF Situation added to Log File

2) Thermal Cut slow And Fast Timers Added to Log File

3) Thermal Cut Enable/Disable default position changed to Enabled from UI

4) Thermal Cut Algorithm @ ACIT Library Bug Fixed

5) Outdoor & Indoor Connection info added to USB Interface Temperature window

6) USB Communication temperature Data Update Min/Max Limits Added in order to

prevent Comm. errrors/ Min is -50C and max is 120C

7) USB error rate information added in order to count comm errors

8) Screen Capture bugs Fixed

**09:46:02..Nov 27 2012 to 14:32:54..Nov 27 2012**

1) Plot Snap Chart Track Ball event error fixed

2) Thermal Cut checkBox uncheck problem fixed

3) Data Log screen rearranged

**14:32:54..Nov 27 2012 to 17:04:14..Nov 27 2012**

1) Data Log \*.csv file target min max step final step row fixed

**17:04:14..Nov 27 2012 to 17:00:00..Nov 29 2012**

1) Fan SB Chassis Options Updated according to EEPRom data

2) Fan Algorithms Fixed

**17:00:00..Nov 29 2012 to 16:01:48..Dec 3 2012**

1) Thermal Cut Panel moved to Compessor Menu

2) Code clean has done, renamed functions !!!

**16:01:48..Dec 3 2012 to 15:33:52..Dec 18 2012**

1) Log Chart Logs 3 minutes more after Stop Command from remote

2) Continues Chart is enabled even at Stop !!!

3) Log Chart Clear Button Added

4) Fan Soft Off added

**15:33:52..Dec 18 2012**

1) Log Chart Widht extended when USB Connected

2) Snap chart Disabled instead Log Chart Height Extended

3) Log Chart Shifts to View last 1 hour... Fixed

4) Fan Soft Off added