**Data Logging Information**

Data can be logged as txt file with \*.csv extension so that can be viewed and edited with Excel.

Select File Name From Data Log File Menu to start Logging

Do not attempt to open file while logging goes on. Logging will hang while file is open but will go on whenever the file as closed.

For data Logging there are 3 sampling options 1 second, 2 seconds and 10 seconds. Default is 2 seconds. You can change sampling

option any time when log goes on.

Max 2700 line of txt file is logged. After reaching max line file is fragmentad into next file as xx.001 . For 1 sec sampling one file size

is 45 minutes , for 2 sec 1.30 hours, and for 10 sec is 7.5 hours.

The Maximum Data that is Logged On the Chart is for last 2 hours. After then logging Chart works LIFO.

**About Charts & Graphics**

Charts and Graphics at Acit-Sim like Mollier Diagram and Log Panel is developed by NPlot library. For more refer to below link:

<http://netcontrols.org/nplot/wiki/>

